3196	 The Reactive Typewriter Program	 -character keyboard including alphabetical upper and lower case for good readability. If the machine is restricted to only a single case the lower case is preferred. The reactive typewriter should be portable. the reactive typewriter should operate over any commercially used dial-type telephone voice or telegraph Telex line or over leased nondial telegraph lines interchangeably.
